{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["12月度发供应商"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"12月度发供应商","index":0,"n_rows":114,"n_cols":10,"rows_kept":114,"merged":[[0,0,0,7],[1,0,1,3]],"flags":["formulas_cached_only"]}
["横河煤矿2024年12月份物资采购计划表（常用材料）"]
["编制单位：仓储科"]
["序号","项目序号","使用单位","物料名称","规格型号","计量","数量","备注","报价单价","单位"]
[1,202412001,"掘一","锁具","Φ15.24","套",50,"东翼北回风巷补打锚杆"]
[2,202412002,"掘一","锚杆钻杆","1M","根",60,"东翼北回风巷补打锚杆"]
[3,202412003,"掘一","锚杆钻杆","0.8M","根",60,"东翼北回风巷补打锚杆"]
[4,202412004,"掘一","麻花钻杆","φ16*1800mm","根",40,"东翼北回风巷补打锚杆"]
[5,202412005,"掘一","注水器","Ф42 粗丝","个",20,"东翼北回风巷补打锚杆"]
[6,202412006,"掘一","锚杆钻杆丝接","B19","个",100,"东翼北回风巷补打锚杆"]
[7,202412008,"掘一","锚杆钻头","φ28 合金","个",20,"东翼北回风巷补打锚杆"]
[8,202412010,"掘一","氧气表","YQY-07","块",1]
[9,202412011,"掘一","乙炔表","YQY-07","块",1]
[10,202412012,"掘一","气割枪","G01-100k 3# 青岛华青","把",1]
[11,202412013,"掘一","割嘴","G01-100k 3#","盒",1]
[12,202412014,"机运","拇指滚刷头","10*3cm","个",50,"三采区风水管路除锈刷漆"]
[13,202412015,"机运","拇指滚刷手柄","L=43cm","个",20,"三采区风水管路除锈刷漆"]
[14,202412016,"机运","滚刷","300mm","个",40,"三采区风水管路除锈刷漆"]
[15,202412017,"机运","毛刷","50mm","个",50,"三采区风水管路除锈刷漆"]
[16,202412018,"机运","百叶片","100*16*72mm","个",50,"三采区风水管路除锈刷漆"]
[17,202412019,"机运","碗型钢丝轮","36*16*80mm","个",100]
[18,202412020,"通巷","记号笔","得力 加粗1.8mm\n蓝色、黑色各20支","支",40,"井下各类牌板填写使用"]
[19,202412021,"通巷","砂轮百叶片","100*16*72mm","片",50,"设备设施打磨除锈使用"]
[20,202412022,"通巷","槽轮滑轮","1.2寸 U 型","个",20,"通风设施加工联锁绳吊挂滑轮使用"]
[21,202412023,"通巷","垫圈","DN100","套",20,"消防材料库储备物资"]
[22,202412024,"通巷","垫圈","DN89","套",30,"消防材料库储备物资"]
[23,202412025,"通巷","垫圈","DN75","套",60,"消防材料库储备物资"]
[24,202412026,"通巷","圆钉","40mm 樱花牌","kg",20,"通风设施维护维修使用"]
[25,202412027,"通巷","圆钉","80mm 樱花牌","kg",20,"通风设施维护维修使用"]
[26,202412028,"通巷","尼龙扎带","白色 300mm*4mm","根",1000,"日常设施维护消耗"]
[27,202412029,"通巷","管箍","DN20 玛钢镀锌接头\n内丝 六分","个",200,"喷雾装置连接，打钻注浆连接使用"]
[28,202412030,"通巷","焊条","φ3.2 J422","kg",20,"日常加工井下所需物料使用"]
[29,202412033,"通巷","钠石灰","500g/盒","盒",20,"仪器仪表药粉更换用"]
[30,202412034,"通巷","光瓦灯泡","1.5V","个",50,"光瓦配件灯泡更换"]
[31,202412035,"通巷","擦机布","白色 纯棉 10kg/包","kg","20","日常设施维护用"]
[32,202412036,"通巷","快速堵漏王","5KG/包","包",10,"处理井下密闭漏风使用"]
[33,202412037,"通巷","美纹胶带","宽20mm 25m/卷","卷",50,"质量标准化提升刷漆使用"]
[34,202412042,"通巷","钢锯条","300mm  细齿","根",50,"日常工作开展使用"]
[35,202412043,"通巷","红胶管","光干涉式甲烷测定器（CJG10）橡胶管软胶","米",15,"光干涉式甲烷测定器连接胶管更换"]
[36,202412044,"通巷","气瓶减压器","防震合金\n 8L气样气瓶","个",2,"仪器维修室气样气瓶安装使用"]
[37,202412045,"通巷","法兰止回阀","H41H-16\n DN100铸钢重型","个",2,"清撒煤巷排水用"]
[38,202412047,"通巷","束管","φ8","米",2000,"东翼北束管铺设"]
[39,202412048,"通巷","束管接头","φ8","个",100,"日常维护束管使用"]
[40,202412049,"通巷","高速风表","DFA-4","块",2,"井下测风工作"]
[41,202412050,"通巷","中速风表","DFA-2","块",2,"井下测风工作"]
[42,202412051,"通巷","微速风表","DFA-3","块",2,"井下测风工作"]
[43,202412054,"运转","干粉灭火器","推车式、35kg、灭火剂：磷酸二氢铵（75%）、硫酸铵（25%），灭火级别：6A 183B","台","4","35kV变电所"]
[44,202412055,"运转","聚氨酯保温管","DN159(卡壳式)","米","50","冬季供暖维修"]
[45,202412056,"运转","聚氨酯保温管","DN133(卡壳式)","米","50","冬季供暖维修"]
[46,202412057,"运转","铝箔开口保温管","6分、管厚20mm","米","300","冬季供暖维修"]
[47,202412058,"运转","铁丝","14#","kg","20","冬季供暖维修"]
[48,202412059,"运转","自动放风","DN20","个","10","冬季供暖维修"]
[49,202412060,"运转","手动放风","暖气片用","个","20","冬季供暖维修"]
[50,202412061,"运转","HP合成抗磨高温复合脂","锐捷安、-30--220℃、2kg/盒","盒","6","抽、压风机"]
[51,202412062,"运转","LED环形灯灯芯","36W、磁吸式","个","10","日常维修消耗"]
[52,202412063,"运转","LED灯条","36W、磁吸式","个","10","日常维修消耗"]
[53,202412064,"运转","液位传感器","DC24V 量程0-20m 带煤安","个","3","-258泵房"]
[54,202412065,"运转","UPS电源","invt BATTERY BOX","个","2","应急电源用"]
[55,202412066,"运转","UPS电源","SANTAK","个","1","应急电源用"]
[56,202412068,"运转","消防阀门接头","DN50、带胶垫","套","5","消防设施"]
[57,202412076,"运转","高压法兰闸阀","DN100 铸钢、1.6Mpa","个",4,"井下主回风系统"]
[58,202412077,"运转","法兰片","DN100、1.6Mpa","片",20,"井下主回风系统"]
[59,202412078,"运转","钢垫","DN100、1.6Mpa","片",500,"井下主回风系统"]
[60,202412079,"运转","结构胶",null,"管",10,"井下主回风系统"]
[61,202412082,"运转","槽钢","100mm","米","300","井下主回风系统"]
[62,202412083,"运转","螺纹钢","DN22","米","300","井下主回风系统"]
[63,202412085,"运转","空压机油","DGV-250A 18L/桶","升","126","空压机"]
[64,202412086,"皮带","角铁","75×75","kg",600,"—160更换皮带大架子"]
[65,202412087,"皮带","角铁","4×4","kg",100,"—160更换皮带大架子"]
[66,202412088,"皮带","角铁","5×5","kg",100,"—160更换皮带大架子"]
[67,202412089,"皮带","镀锌铁丝","8#","kg",300,"—160更换皮带机头"]
[68,202412090,"皮带","镀锌铁丝","14#","kg",200,"—160更换皮带机头"]
[69,202412091,"皮带","钢丝绳卡子","20#","个",20,"—160更换皮带机头"]
[70,202412092,"皮带","除锈剂","500ml/瓶","瓶",30]
[71,202412093,"机厂","防冻液","18KG/桶","桶",2,"叉车使用"]
[72,202412094,"机厂","空气滤芯","合力叉车","个",2,"叉车维修"]
[73,202412096,"调度室","监控传输线","MHYV1X4X7/0.52","米",1000,"井下监测监控用"]
[74,202412097,"调度室","矿用网线","MHYVP4X2*0.58","米",500]
[75,202412099,"调度室","矿用本安电话机","KTH15","台",10,"井下通讯"]
[76,202412101,"调度室","电源适配器","液晶显示器专用AC220V-DC12V","个",5,"显示器用"]
[77,202412102,"调度室","户外式定阻高音喇叭","500mm*500mm\n-50W-16Ω","个",2,"地面广播用"]
[78,202412103,"调度室","冷补胶","LBJ_200","箱",1]
[79,202412104,"调度室","PVC防水胶布",5,"盘",30]
[80,202412105,"调度室","标准气样","甲烷3.0%\\8L","瓶",1,"监测监控校验"]
[81,202412106,"调度室","标准气样","甲烷2.0%\\8L","瓶",3,"监测监控校验"]
[82,202412107,"调度室","标准气样","甲烷0.5%\\8L","瓶",1,"监测监控校验"]
[83,202412108,"调度室","标准气样","一氧化碳500ppm\\8L","瓶",3,"监测监控校验"]
[84,202412109,"调度室","标准气样","二氧化碳2.0%\\8L","瓶",2,"监测监控校验"]
[85,202412110,"调度室","标准气样","氧气14.9%\\8L","瓶",2,"监测监控校验"]
[86,202412111,"调度室","标准气样","纯氮气100%\\8L","瓶",2,"监测监控校验"]
[87,202412112,"调度室","标准气样","空气20.9%\\8L","瓶",1,"监测监控校验"]
[88,202412032,"通巷","甲烷标准气样","1.0% 8L/瓶","瓶",1,"仪器仪表标校使用"]
[89,202412113,"救护队","HYZ4氧气呼吸机","山西虹安","台",2]
[90,202412114,"救护队","隔绝式压缩氧自救器","ZYX45","台",10]
[91,202412115,"煤场","翻斗油缸密封件","英轩656HN","套",3,"铲车维修"]
[92,202412116,"煤场","举升油缸密封件","英轩656HN","套",3,"铲车维修"]
[93,202412117,"煤场","转向油缸密封件","英轩656HN","套",3,"铲车维修"]
[94,202412118,"煤场","翻斗油缸密封件","龙工LG855B","套",1,"铲车维修"]
[95,202412119,"煤场","举升油缸密封件","龙工LG855B","套",1,"铲车维修"]
[96,202412120,"煤场","转向油缸密封件","龙工LG855B","套",1,"铲车维修"]
[97,202412121,"总务","垃圾袋","45*50","包",20]
[98,202412122,"总务","垃圾袋","60*80","包",20]
[99,202412123,"总务","草酸","25KG/桶","kg",50,"2桶"]
[100,202412131,"通巷","一氧化碳测定器","CTH1000(A)\n防护等级IP65","台",4,"新《煤矿安全规程》规定需更新换新"]
[101,202412132,"通巷","甲烷氧气测定器","CJY4/25(A)\n防护等级IP65","台",6,"新《煤矿安全规程》规定需更新换新"]
[102,202412133,"通巷","氢气检测报警仪","测量范围：0-1000ppm\n防护等级IP65","台",2,"井下充电硐室测量气体"]
[103,202412134,"通巷","矿用便携五合一气体检测仪","CH4、CO2、CO、O2、H2S  防护等级IP65\n","台",1,"新《煤矿安全规程》规定需更新换新"]
[104,202412137,"运转","密封圈","38*30mm","个","60","井下变电所"]
[105,202412138,"运转","低压智能馈电保护装置","ALDB-ME","个","1","井下变电所"]
[106,202412139,"运转","高压智能综合保护装置","PIR-I","个","1","高防开关"]
[107,202412140,"运转","户内高压带电显示装置","DXV-Q","个","1","35kV变电所"]
[108,202412163,"运转工区","矿灯房微机控制系统升级改造申请","据上级单位检查要求，我矿矿灯房微机控制系统，共计13灯架，入井人员“三八制”“四六制”不能独立显现。人员升井后2小时不交矿灯不能及时显现，不符合《煤矿安全规程》第四百七十一条第五项规定，需对该系统进行升级改造，请领导审批。","次","1"]
[109,202412164,"采一工区","综采液压支架系统调试","支架系统出现故障要求厂家四川航天电液控有限公司技术人员来矿入井调试","次","1"]
[110,202412128,"采一","调高阀组组件","SM87YT4-0201","件",2,"检查问题整改项采煤机用（加工周期约3个月）月度中标价"]
[111,null,"通巷","便携式激光甲烷检测报警仪","JJB10\n防护等级IP65","台",2]